IOM441W-S 

Relay module IOM441W-S is used to extend isolation fault location systems such as EDS44x with 12 potential free contacts.

IOM441W-S, Art.-No.: B95012057W

Supply voltage: Via BB-Bus Interface

Dimensions (WxHxD): 72 mm x 93 mm x 63 mm

Operating temperature: -40...70° C

Degree of protection, internal components: IP 40

Degree of protection, terminals: IP 20

Indicators: LED: Operation

Interfaces:
BB bus (specific sensor bus for din rail)
12 separately adjustable potential-free NO contacts (NC, NO selectable)
3 functions can be assigned to each relay.

Connection:
Push-wire terminals

Manufacturer:
Bender GmbH & Co. KG
Londorfer Straße 65
35305 Grünberg

Type: IOM441W-S
Article number: B95012057W
Unit: piece