COMTRAXX® RCP115
Remote Control Panel 15.6‘‘ – for displaying and controlling web-based visualizations

Description:

The COMTRAXX® RCP115 is an industrial 15.6" touch panel designed for displaying web-based visualizations. It enables the visualization of condition monitoring applications from the COMTRAXX® product range as well as visualizations from third-party manufacturers via standardized web interfaces.
The panel is equipped with a powerful processor, making it suitable for complex visualizations with high graphical load and animated content, which are displayed smoothly and without lag.
Via the integrated interface, up to four different visualization accesses can be configured. The system supports both static IP addressing and operation in DHCP mode.
To protect against unauthorized changes, device and network settings can only be modified via a password-protected access level.
The touch panel can be seamlessly integrated into existing IT and automation networks via its Ethernet interface.

To ensure the safe operation of the Remote Control Panel after delivery, a structured process for handling potential vulnerabilities has been established. This process includes the reporting, assessment, and, where necessary, remediation of security-relevant incidents.
Further information about our security process can be found on our website:
https://www.bender.de/cert


Gerätemerkmale:

· Device type: Multitouch remote control panel with Ethernet interface
· Housing: Anodized aluminum housing with glass front
· Display:
· Glass thickness: 3 mm
· Display size, resolution: 15.6" 1920 × 1080 px (16:9)
· Backlight: 800 cd/m²
· Colors: 24-bit RGB
· Touchscreen: Multi-touch PCAP (Projected Capacitive Touch)
· Interfaces:
· RJ45 Ethernet: 10/100/1000 Mbit/s
· USB: USB 2.0 Hi-Speed host
· Cooling: Passive, no rotating parts
· Power supply: 24 V DC (±15%)
· Operating temperature: 0 to +50 °C
· Relative humidity: 95%, non-condensing
· Degree of protection: Front IP65, Back of the device: IP20
· Installation: Mounted using clamping brackets attached to the rear of the panel
· Approvals: CE, UKCA

Mechanical data:
Dimensions (W x H x D): 425.16 x 274.59 x 33 mm
Cutout dimensions: 393 x 242 mm
Glass thickness: 3 mm
Weight: 3840 g
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